Distributor Removal. Buick Roadmaster 1996

For 1990-2009 cars

1. Disconnect the spark plug harness from the spark plugs.
2. Disconnect the ignition harness from the ignition coil. Do not remove the wires from the distributor unless it is necessary.

Important: Do not allow foreign material to enter the open vacuum lines. Cap the ends if necessary.

3. Disconnect the vacuum harness.
4. Remove the distributor bolts.
5. Remove the distributor.