SMU - SECTIONS 10-5, 10-6, & 10-8 - EXTERIOR FENDER. Buick Roadmaster 1995

For 1990-2009 cars

# SMU - SECTIONS 10-5, 10-6, & 10-8 - EXTERIOR FENDER

---------------------------------------------------------------------- SERVICE MANUAL UPDATE ----------------------------------------------------------------------

#### SUBJECT: SECTIONS 10-5, 10-6 AND 10-8 - EXTERIOR FENDER, DOOR AND REAR QUARTER CENTER MOLDINGS

#### MODELS: 1995 BUICK ROADMASTER SEDAN

PROPER INSTALLATION OF THE BODY SIDE MOLDINGS IS CRITICAL TO THE ADHESION DURABILITY OF THESE PARTS.

THE VERTICAL POSITION IS IMPORTANT, AS IT ALLOWS FULL CONTACT OF THE ADHESIVE STRIP TO THE BODY CONTOURS. CLEAN SURFACES AND PROPER ROLLING TECHNIQUE ALLOW DESIGN INTENTION TO BE ACHIEVED.

THE INFORMATION IN THIS BULLETIN IS FROM A SUPPLEMENT TO THE 1995 SERVICE MANUAL. THE FIRST PRINTING OF THE MANUAL DID NOT COVER THE NEW ADHESIVE MOUNTED MOLDINGS.

FIGURES: 0 ATTACHMENTS: 4

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.