OIL LEAKS FROM REAR OF ENGINE (REPLACE PLUG). Buick Roadmaster 1992

For 1990-2009 cars

# OIL LEAKS FROM REAR OF ENGINE (REPLACE PLUG)

#### SUBJECT: OIL LEAKS FROM REAR OF ENGINE (REPLACE CAMSHAFT PLUG)

#### MODELS AFFECTED: 1992 ROADMASTER

#### CONDITION:

---------

Some owners of 1992 Roadmasters may comment on oil leaks from the rear of the engine. Some of these leaks may be misdiagnosed as a rear main crankshaft seal or oil pan gasket leak.

#### CAUSE:

-----

Insufficient sealant around the camshaft plug, P/N 3997752, at the rear of the engine block.

#### CORRECTION:

----------

Before making repairs for rear main crankshaft seal or oil pan gasket leaks, check the cam plug by disconnecting the transmission and visually inspecting for oil leaks around the cam plug. Replace the plug if necessary. Use the following procedure to install a new plug.

- Coat plug outside diameter with GM part number 12346004 sealant or equivalent.

- Install plug flush to 0.79 mm (1/32 inch) deep.

Parts are currently available from GMSPO.

#### WARRANTY INFORMATION:

Labor Operation No.: J1660 Labor Time: 2.1 hrs.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.