Oil Pump Body Bushing Replacement. Buick Roadmaster 1996

For 1990-2009 cars

#### Tools Required

• | J 41778-1 Pump Body Bushing Installer/Remover

• | J 41778-2 Pump Body Bushing Position Stop

1. Inspect the oil body for the following defects:

• | Worn or damaged bushings

• | Foreign material or debris

• | Porosity

• | Scored or irregular mating faces

• | Cross channel leaks

• | Ring groove damage

2. Remove the front helix retainer.
3. Remove the oil seal assembly.
4. Remove the pump body bushing.
5. Using J 41778-1 , install the pump body bushing.
6. Use J 41778-2 for a proper bushing depth.