Cylinder Head Removal. Buick Roadmaster 1996

For 1990-2009 cars

1. Remove the engine coolant air bleed pipe bolts, pipe, and sealing washers.

Use a backup wrench on the pipe fitting when you remove the bolts.

2. Remove the ignition coil and the ignition coil bracket from the cylinder head.
3. Remove the cylinder head bolts.

Notice: After removal, place the cylinder head on 2 wood blocks in order to prevent damage to the sealing surfaces.

4. Remove the cylinder head.
5. Remove and discard the gasket.