Starter Disassemble. Buick Roadmaster 1996

For 1990-2009 cars

1. Disassemble the nuts and the heat shield from the clamp bolts/screws.
2. Disassemble the nut and field lead from the solenoid switch.
3. Disassemble the clamp bolts/screws and the solenoid switch with clamp from the drive housing.
4. Disassemble the bolts/screws from the starter motor.
5. Disassemble the commutator end frame, the brake washer, and the frame kit from the armature and the drive housing.
6. Disassemble the plug from the drive end housing.
7. Disassemble the armature with the starter drive, the shift lever, the plunger, and the starter solenoid switch plunger spring from the drive housing.
8. Disassemble the starter solenoid switch plunger spring from the plunger.
9. Disassemble the plunger from the shift lever.
10. Disassemble the shift lever from the drive housing by spreading the lever arms slightly to disengage.
11. Disassemble the thrust collar from the armature shaft.
12. Disassemble the retainer by pushing the starter drive stop collar off of the retainer and sliding it off of the armature shaft.
13. Discard the retainer.
14. Disassemble the starter drive stop collar and the starter drive from the armature shaft.
15. Inspect the starter motor components. Refer to Starter Motor Inspection .