Evaporative Emission Canister Purge Solenoid Valve Replacement. Buick Roadmaster 1996

For 1990-2009 cars

### Removal Procedure

1. Disconnect the electrical connector
2. Disconnect the hoses (4) from the solenoid valve (1).
3. Remove the bracket and solenoid (1) from the intake manifold (2).

### Installation Procedure

1. Install the solenoid valve (1) to the intake manifold (2).

Tighten
Tighten the Fastener to 5.8 N·m (52 lb in).

2. Connect the electrical connector to the solenoid valve (1).
3. Connect the hoses to the solenoid valve (1).