Intake Manifold Removal. Buick Roadmaster 1996

For 1990-2009 cars

1. Remove the accelerator cable bracket bolts and bracket.
2. Remove the throttle body bolts, gasket and throttle body.
3. Remove the crankcase vent hose.
4. Remove the EGR valve, gasket and nuts.
5. Discard the EGR valve gasket.
6. Disconnect the fuel pressure regulator vacuum hose.
7. Remove the air cleaner resonator bracket bolts..
8. Remove the air cleaner resonator bracket.
9. Remove the fuel rail bolts and fuel rail with injectors.
10. Remove the intake manifold bolts and studs.
11. Remove the intake manifold assembly.
12. Remove and discard the gaskets.