3rd Accumulator Retainer with Ball Assembly Leak Check. Buick Roadmaster 1996

For 1990-2009 cars

### Installation Procedure

#### Tools Required

J 29714-A Servo Cover Compressor

1. Install the 2-4 servo into the case.
2. Use the J 29714-A in order to compress the servo cover.
3. Install the servo cover retaining ring.
4. Pour the solvent into the accumulator bore until the channel is filled. Watch for leaks in the case channel.
5. If leakage is observed, replace the third accumulator retainer and ball assembly.