Reverse Input Clutch Assemble. Buick Roadmaster 1996

For 1990-2009 cars

#### Tools Required

• | J 23327 Clutch Spring Compressor

• | J 25018-A Clutch Spring Compressor Adaptor

1. Inspect the reverse input piston for the following defects:

• | Damaged or porosity

• | Ring groove damage

2. Install the reverse input clutch inner and outer seals on the piston.
3. Install the reverse input piston into the reverse input clutch housing and drum assembly.
4. Inspect the reverse input clutch spring assembly or distortion or damage.
5. Install the reverse input clutch spring assembly.
6. Install the clutch spring compressor.
7. Install the reverse input clutch spring retainer ring.
8. Inspect the composition plates, the steel plates and the backing plates for the following items:

• | Damaged tangs.

• | Delamination.

• | Excessive wear.

• | Heat damage or wear.

• | Surface finish.

• | Flatness.

9. Install the reverse input clutch belleville plate into the reverse input clutch housing and drum assembly.
10. Install the reverse input clutch plates starting with a steel plate and alternate with a composition plate.
11. Install the reverse input clutch backing plate.
12. Install the reverse input clutch retaining ring.