Exhaust Manifold Removal. Buick Roadmaster 1996

For 1990-2009 cars

## Exhaust Manifold Removal Right Side

1. Remove the secondary air injection pipe and check valve from the exhaust manifold. Do not remove the check valve from the pipe unless necessary.
2. Remove the EGR inlet pipe, gasket and bolts.
3. Remove the studs and the bolts from the right exhaust manifold.
4. Remove the exhaust manifold.
5. Remove the exhaust manifold gasket.
6. Discard the gasket.

## Exhaust Manifold Removal Left Side

1. Remove the secondary air injection pipe and check valve from the left exhaust manifold. Do not remove the check valve from the pipe unless necessary.
2. Remove the studs and the bolts from the left exhaust manifold.
3. Remove the exhaust manifold.
4. Remove the exhaust manifold gasket.
5. Discard the gasket.