Oil Level Indicator and Tube Installation. Buick Roadmaster 1996

For 1990-2009 cars

1. Apply sealant GM P/N 12346004 or equivalent around the oil level indicator tube 13 mm (0.5 in) below the tube bead.
2. Install the oil level indicator tube into the engine block. Rotate the oil level indicator tube into position.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the oil level indicator tube bolt.

Tighten
Tighten the oil level indicator tube bolt to 12 N·m (106 lb in).

4. Install the oil level indicator into the oil level indicator tube.