MANUAL SEAT ADJUSTER LATERAL MOVEMENT. Buick Skyhawk 1984

For 1990-2009 cars

# MANUAL SEAT ADJUSTER LATERAL MOVEMENT

#### Models Affected: 1983 & 1984 Skyhawk (Except Easy Entry)

#### NOTICE: This bulletin supersedes 84-10-26 dated February, 1985, to provide part numbers for the passenger side outer adjusters. Please discard original bulletin and replace it with this one.

If a lateral movement of the inner seat adjuster is experienced, perform the following operations.

1. Remove seat and place on a clean protected surface.

2. Replace seat adjuster(s) with new adjuster(s).

P/N 20329374 Passenger Outer(Coupe) P/N 20329375 Passenger Outer(Sedan) P/N 20162884 Passenger Inner(Coupe) P/N 20162885 Passenger Inner(Sedan) P/N 20330804 Driver's Inner(Coupe) P/N 20330805 Driver's Inner(Sedan)

3. Install release wire (P/N 20162898) between lock bars.

4. If the adjuster to floor attaching stud is loose in the floor, weld the stud (mig or gas with steel rod only) into place using standard body shop repair procedure for structural components.

5. Install seat to floor and torque seat adjuster-to-floor pan attaching nuts 20 to 28 N.m (15 to 21 ft. lb.).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.