EXHAUST MANIFOLD CRACKING NEW MANIFOLD AVAILABLE. Buick Skyhawk 1982

For 1990-2009 cars

# EXHAUST MANIFOLD CRACKING NEW MANIFOLD AVAILABLE

SOME 1982 1.8L L4 ENGINES MAY INCUR CRACKED EXHAUST MANIFOLDS WHEN SUBJECTED TO HIGH TEMPERATURE AND HIGH LOAD CONDITIONS. A NEW EXHAUST MANIFOLD ASSEMBLY HAS BEEN RELEASED UNDER THE OLD PART NUMBER. EARLY DESIGN PARTS ARE NO LONGER IN STOCK. REPLACEMENT OF THE EXHAUST MANIFOLD ASSEMBLY REQUIRES A CHANGE IN THE OUTER BOLT (#1 AND #4 RUNNERS) TORQUE SPECIFICATION. THESE BOLTS SHOULD BE TORQUED TO 15-20 N.M(11-15 FT).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.