NEW VEHICLE ANNOUCEMENT INFORMATION. Buick Skyhawk 1986

For 1990-2009 cars

# NEW VEHICLE ANNOUCEMENT INFORMATION

#### MODELS AFFECTED: ALL 1986 BUICKS

1. 1986 Warranty and Owner Assistance Information Booklets 2. 1986 Buick Service Manuals 3. 1986 Buick Owner's Manuals 4. 1986 Vehicle Certification and Tire Pressure Label 5. 1986 New Vehicle Inspection Procedure Sheets 6. 1986 Buick Passenger Car Maintenance Schedule Booklet 7. 1986 Buick Labor Time Guide 8. 1986 Buick Bulletin Binders 9. 1986 Paint Codes

1. WARRANTY AND OWNER ASSISTANCE ON 1986 BUICK NEW CARS ------------------------------------------------------- The following booklets containing warranty information relative to the new car, emission systems, tire and corrosion are used in 1986:

Part #25524019 - Riviera Part #25527756 - Electra and Park Avenue FWD Part #25521843 - Somerset/Skylark (Built Prior to September 23, 1985)

Part #25527716 - All Except Riviera, Electra/Park Avenue FWD and Somerset/Skylark (Built Prior to September 23, 1985) (Can be and may have been used in place of 25521843 for Somerset/Skylark built prior to September 23, 1985)

Part #25528305 - All Except Riviera & Electra/Park Avenue FWD (Replaces 25521843 & 25527716 on cars built after September 23, 1983, and may be used for cars built prior to September 23, 1985)

Owner assistance satisfaction procedures, the mediation/arbitration prograrm, special policy adjustment prograrns, and the GM Continuous Protection Plan are all outlined in this booklet. A separate tire warranty folder is included to outline warranty as provided by individual tire manufacturers.

The owner's name, address, Vehicle Identification Number, date of delivery and mileage at the time of delivery, are all to be typed on the front cover of the Warranty and Owner Assistance Information booklet in the space provided. There is a space provided on the back of the folder for the dealer name, address and dealer code.

It is very important that the Owner and Vehicle Information on the booklet be correct. This information will be the only means of owner identification for repairs covered under warranty. In order for dealer warranty claims to be properly processed, the Vehicle Identification Number must be correct. Owners should be instructed to carry their Warranty and Owner Assistance Information Booklets in their vehicles at all times.

2. 1986 SERVICE MANUALS ----------------------- The 1986 Chassis Service Manual will be shipped to all Buick dealers in early September, 1985. Again for 1986 it is a loose-leaf publication in two volumes, covering all models.

Post type binders will be included with each manual.

1986 Fisher Body Manual will be shipped in mid-September, 1985.

Additional manuals and/or binders can be ordered on the "Service Publications for Buick Dealers" order form which is included with the Chassis Service manual shipment.

3. 1986 OWNER'S MANUALS ----------------------- For 1986 there are a total of eight (8) owner's manuals.

Part # 25524011 - Century Part # 25524811 - LeSabre Estate Wagon/Electra Estate Wagon Part # 25524016 - Electra/Park Avenue Part # 25528093 - Riviera (Replaces - 25521462 used on early built cars) Part # 25524012 - Regal Part # 25520381 - LeSabre Part # 25524013 - Skyhawk Part # 25523809 - Somerset/Skylark

For Electra/Park Avenue the suede finish wallet, part nunber 25518866 has been discontinued.

4. 1986 VEHICLE CERTIFICATION AND TIRE PRESSURE LABEL ----------------------------------------------------- In accordance with Federal Motor Vehicle Regulations, A Vehicle Certification and Tire Pressure Label is being affixed to all 1986 model Buicks.

The label will have a certification statement, Vehicle Identification Number, month and year that the vehicle was built. The label will be attached horizontally to the left front door inner panel lock facing on all models.

The lower portion of the label will have the tire size and tire pressure information.

Due to the ceritification label's location, it may be subject to damage during car shipment and new vehicle pre-delivery service or may be required due to door repair or replacement.

To acquire a replacement certification label, proceed as follows:

A. Obtain an impression of the Vehicle Identification Number on the engine block by rubbing a pencil lightly over a piece of paper held in place against the block.

B. Obtain build date, if at all possible, from damaged certification label.

C. Check Vehicle Identification Number on engine block and identification number on instrument panel to see that they match.

D. Obtain the vehicle order number from invoice.

E. Send the readable impression and build date from Steps A and B above and the vehicle order number taken from the invoice, along with a letter of explanantion to:

Buick Motor Division Attn: Manager - Technical Service Flint, MI 48550

5. 1986 NEW VEHICLE INSPECTION PROCEDURE FORM ---------------------------------------------

The New Vehicle Inspection and Delivery Procedure which was introduced in 1983, includes a new NVI for 1986. Use New Vehicle Inspection Procedure Sheet 101072. This form is shipped with each Buick delivered to you. Additional forms may be obtained through your Zone Office.

6. 1986 MAINTENANCE SCHEDULE ---------------------------- For 1986 there is one (1) vehicle maintenance booklet for all cars, part number 14085242.

7. 1986 LABOR TIME GUIDE - MICROPUBLICATIONS UPDATE AND REQUEST FOR REVIEW FORMS

Approximately September 16, 1985, one (1) set of micropublications will be mailed to all dealers, each set will consist of the following material:

o Labor Time Guide - 1986 (2)

o Dealer Technical Bulletin Update - October 1983-August 1984 (1)

o Dealer Information Bulletin Update - October 1983-August 1984 (3)

o Dealer Service Bulletin Update - All 1984 (1)

o Dealer Campaign Bulletin Update - October 1983-August 1984 (2)

o Essential/Available Tool Catalog Update - 1984 (1)

o Chassis Service Mamual - 1984 (1)

Additional quantities, if previously ordered, will be supplied, based upon records on file at time of mailing. All requests for additional microfiche sets are to be processed directly thru GM Photographic. Additional order forms are available from your Zone Office.

Labor Time Guide - All claims processed on the date of receipt or after will be processed on the basis of operations and labor time allowances provided.

#### Printed Labor Time Guide

The 1986 Labor Time Guide is available in printed format. This loose leaf publication can be ordered on the "Service Publications for Buick Dealers" order form. Binders are now also available. Printed Labor Time Guides will automatically be sent to dealers who have previously ordered on a continuing basis.

8. 1986 BUICK BULLETIN BINDERS ------------------------------- Orders for binders and index tabs should be sent directly to Buick Motor Division in care of Office Service Department, as shown on the order form included with this Bulletin. Binders can also be ordered using the "Service Publication for Buick Dealers" order form.

9. 1986 PAINT CODES ------------------- Color chip sheets for the 1985 Buick Paints will again be available from DuPont, Ditzler, Inmont (Rinshed-Mason), Sherwin Williams, Acme/Rogers and Martin-Senour.

The following chart indicates 1986 exterior paint supplier stock number, the Fisher WA numbers and vehicles the paint is used on. The paint numbers listed in this bulletin along with clearcoat materials, are or soon will be available from local paint suppliers. Please note that the Service Parts Label includes paint information.

When contacting your local paint supplier for repair materials, make sure that you specify the type of material needed. If your paint supplier is unable to provide you with the material needed, ask him to contact his manufacturer sales representative for assistance.

#### NOTICE: All 1986 Centurys built at the Oklahoma City Assembly Center (plant code 6) will be basecoat/clearcoat although paint codes shown are lacquer codes. Formulation of some of these paints will be specific. Work is in process to determine which colors need specific formulation. A bulletin with this information will be released as soon as paint refinish information is available. INMONT/ PAINT FISHER SERIES PPG RINSHED CODE COLOR WA# USAGE DITZLER DUPONT MASON ---- ----- ------ ------ ------- ------ ----- 11 WHITE 3967 A,G,J,B-WAGON 2058 5338 2080

12 SILVER * 8535 A,G,J,B-WAGON 3746 B8501 15001 13S SILVER B/C * 9021 C,E,H,N 3822 D8590 15365 15 MED. GRAY * 8573 A,G,J,B-WAGON 3749 B8502 15004 17 BIACK B/C * 8523 N 3752 B8537 15007G 19 BLACK 848 A,G,J,B-WAGON 9300 99S A946

22 LT.BLUE B/C * 8533 C,E,H,N 3753 B8538 15008F 24 MED.BRIGHT BLUE * 8928 J 3883 B8601 16002 25 LT. BLUE * 8574 A,G,J,B-WAGON 3754 B8503 15009 27 MED.BLUE B/C * 8532 N 3756 B8539 15048V 29 DK. BLUE B/C * 8540 C,E,H 3757 B8547 15011D 31 DK. BLUE * 8592 A,G,J,B-WAGON 3760 B8504 15014 40 WHITE B/C 8554 C,E,H,N 3680 B8469 13570 41 BLACK B/C 8555 C,E,H 9700 99S 13572 42 LT. SAGE B/C * 8521 N 3761 B8540 15015G 43 LT. SAGE * 8572 A,G,B-WAGON 3762 B8505 15016 48 BLACK EMERALD B/C * 8747 C,E,H 3888 B8608 16006 49 DK. SAGE B/C * 8612 N 3765 B8541 15019F 52 SEDONA TAN B/C 8528 N 3768 B8542 15022 54 YELLOW BEIGE 8525 A,G,J,B-WAGON 3769 B8521 15023 58 LT. CHESTNUT * 8575 A,G,J,B-WAGON 3772 B8507 15026 61 LT. CHESTNUT B/C * 8566 H,N 3775 B8543 15029G 62 DK. CHESTNUT * 8593 A,G,J,B-WAGON 3776 B8508 15030 63 LT. DRIFTWOOD B/C 8744 C,E,H 3894 B8603 16011 64 DK. CHESTNUT B/C * 8567 H,N 3777 B8544 15031G 65 MED. DRIFTWOOD B/C* 8745 C,E 3895 B8604 16012F 70 CARMINE 8530 J 3781 B8512 15035V 71 MED.RED * 8772 A,G,B-WAGON 3899 B8602 16016D 74 FLAME RED B/C * 8748 C,E,H,N 3823 B8610 16017 75 GARNET RED 8746 C,E 3900 B8606 16018 FIREMIST B/C * 78 DK.CARMINE B/C * 8756 H 3901 B8624 16019 79 DK.RED * 8529 A,G,J,B-WAGON 3786 B8509 15040M 84 GUNMETALMB/C * 7782 C,E,H,N 3667 B8403 14066D 90 WHITE DIAMOND B/C 8933 E 3903 B8609 16021 92 MED.RMERALD B/C * 8931 E 3904 B8607 16022G 94 MED.BLUE FIREMIST 8545 C,E 3792 B8549 15046D B/C * 96 DK.DRIFTWOOD 8765 C,E 3906 B8605 16024G FIREMIST B/C * 99 BLACK CHERRY B/C * 8244 E 3673 B8414 14071D

B/C - BASECOAT/CLEARCOAT * METALLIC

PAINT SHERWIN-WILIAMS MARTN CODE COLOR (ACME-ROGERS) SENOUR ---- ----- ------------- ------ 11 WHITE LlOA-2864 30-3929 (5644)

12 SILVER * 34380 30-5371 13S SILVER B/C * 35369 30-5491 15 MED. GRAY * 34381 30-5372 17 BIACK B/C * 34421 30-5409 19 BLACK LlOB-1738 3069 (3000/4590)

22 LT.BLUE B/C * 34383 30-5374 24 MED.BRIGHT BLUE * 35252 30-5471 25 LT. BLUE * 34382 30-5373 27 MED.BLUE B/C * 34384 30-5375 29 DK. BLUE B/C * 34385 30-5376 31 DK. BLUE * 34875 30-5441 40 WHITE B/C 33755 30-5295 41 BLACK B/C 33756 30-5296 42 LT. SAGE B/C * 34387 30-5378 43 LT. SAGE * 34386 30-5377 48 BLACK EMERALD B/C * 35315 30-5482 49 DK. SAGE B/C * 34390 30-5381 52 SEDONA TAN B/C 34392 30-5383 54 YELLOW BEIGE 34861 30-5437 58 LT. CHESTNUT * 34396 30-5387 61 LT. CHESTNUT B/C * 34397 30-5388 62 DK. CHESTNUT * 34398 30-5389 63 LT. DRIFTWOOD B/C 35310 30-5481 64 DK. CHESTNUT B/C * 34399 30-5390 65 MED. DRIFTWOOD B/C* 35317 30-5483 70 CARMINE 34401 30-5392 71 MED.RED * 35319 30-5484 74 FLAME RED B/C * 35320 30-5485 75 GARNET RED 35278 30-5477 FIREMIST B/C * 78 DK.CARMINE B/C * 35321 30-5526 79 DK.RED * 34405 30-5396 84 GUNMETALMB/C * 33936 30-5313 90 WHITE DIAMOND B/C 35424 30-5528 92 MED.RMERALD B/C * 35255 30-5474 94 MED.BLUE FIREMIST 34411 30-5402 B/C * 96 DK.DRIFTWOOD 35324 30-5486 FIREMIST B/C * 99 BLACK CHERRY B/C * 33941 30-5337

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.