ENGINE OIL PRESSURE SWITCH REMOVAL INFORMATION-1.8L. Buick Skyhawk 1982

For 1990-2009 cars

# ENGINE OIL PRESSURE SWITCH REMOVAL INFORMATION-1.8L

1982 and 1983 Skyhawks without a gage package and equipped with a 1.8L OHC engine (VIN Code 0) require a special socket for removal of the oil pressure sending switch. This socket is available from Kent-Moore Tool Division, number J-21757-03. Mac Tools, number SC-46 or Snap-On Tools, number A-119A.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.