REVISED: AIR DEFLECTOR REPAIR LOOSE SIDE. Buick Skyhawk 1982

For 1990-2009 cars

# REVISED: AIR DEFLECTOR REPAIR LOOSE SIDE

#### MODELS AFFECTED: 1982 Skyhawk

This Bulletin supersedes Bulletin 82-T-111A. The Labor Operations on 82-T-111A are incorrect. Please discard 82-T-111A and replace it with 82-T-111B.

The side air deflector on a 1982 Skyhawk may be pulled loose when backing away from a snowbank or a curb. Should this condition occur, repair as follows:

1. Raise car on hoist.

2. Drill a 1/8" hole in the side air deflectors, and front end panel while holding the two parts in place (See Illustration).

3. Install a 1/8" pop-rivet and washer as shown in Illustration.

4. Lower Car.

WARRANTY INFORMATION

LABOR OPERATION B0460 RIGHT B0461 LEFT

TIME ALLOWANCE 0.2 HRS.

TROUBLE CODE: 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.