ERRATIC HORN OPERATION. Buick Skyhawk 1985

For 1990-2009 cars

# ERRATIC HORN OPERATION

#### Vehicles Affected: 1985 'J' Models

#### CONDITION:

---------- Some 1965 'J' Models may experience erratic horn operation while the horn pad is depressed.

#### CAUSE:

----- The condition may be caused by an intermittent ground between the horn and chassis attachment.

#### CORRECTION:

----------- Replace the existing attaching J-Nut and bolt with a serrated-type J-Nut and bolt. Use new part numbers 11509595 serrated-type J-Nut and 11502661 bolt for the above described condition. See illustration.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.