FRONT BRAKE DISC LINING CHANGE NON-CHAMFERED PADS. Buick Skyhawk 1984

For 1990-2009 cars

# FRONT BRAKE DISC LINING CHANGE NON-CHAMFERED PADS

#### Models Affected: 1982-1985 Skyhawks and 1985 Somerset Regals

This bulletin supersedes 85-5-2, dated February, 1985.

1982-1984 Skyhawks and some early production 1985 Skyhawks and 1985 Somerset Regals may have been assembled with front brake pads which had a chamfer on the leading and rear edge of the linings. Refer to illustration.

Current production Skyhawks and Somerset Regals are using non-chamfered front disc pads.

Front disc brake noise can be reduced on 1982-1984 Skyhawks, early 1985 Skyhawks and early 1985 Somerset Regals by the installation of non-chamfered disc pads.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.