SPECIAL POLICY: CRACKED EXHAUST MANIFOLD. Buick Skyhawk 1985

For 1990-2009 cars

# SPECIAL POLICY: CRACKED EXHAUST MANIFOLD

#### MODELS AFFECTED: 1985-86 SKYHAWK WITH 2.0L (LQ5) ENGINE (VIN CODE P) AND CALIFORNIA EMISSIONS (NB2)

#### NOTICE: This bulletin is being issued to correct the Exhaust Manifold Seal part number in Bulletin 86-POL-3, dated August, 1989.

The exhaust manifold seal part number should read 14093542 in the Parts Information section of the bulletin. The correct number is shown in the Warranty Claims Information section. Please make the correction to your copies of bulletin 86-POL-3. Dealers were notified of this error by DCS message (DCS Number 89-16) on August 7, 1989.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.