BROKEN A/C COMP. DISCH. PIPE INSTALL BRACKET AND CLAMP. Buick Skyhawk 1986

For 1990-2009 cars

# BROKEN A/C COMP. DISCH. PIPE INSTALL BRACKET AND CLAMP

#### MODELS AFFECTED: 1985-86 SKYHAWKS WITH 2.0L ENGINE (P)

#### NOTE: This bulletin supersedes Bulletin No. 86-1-7 dated June, 1986, for part number correction. Please discard the orginal bulletin and replace it with this one.

Some 1985-86 Skyhawks with 2.0L engines may experience a broken air conditioning compressor discharge pipe. If this occurs, a bracket and clamp to support the muffler is now available to prevent recurrence of the failure. Bracket and clamp support kit, Part Number 22535625 is now available from GMWDD and should be installed. The bracket can be installed by removing the compressor to bracket bolt and installing the bracket and clamp as shown in Illustration.

#### WARRANTY INFORMATION

LABOR OPERATION T4092 LABOR TIME .6 HOURS TROUBLE CODE 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.