MANUAL SEAT ADJUSTER LATERAL MOVEMENT. Buick Skyhawk 1983

For 1990-2009 cars

# MANUAL SEAT ADJUSTER LATERAL MOVEMENT

IF A LATERAL MOVEMENT OF THE INNER SEAT ADJUSTER IS EXPERIENCED, PERFORM THE FOLLOWING OPERATIONS: 1. REMOVE SEAT AND PLACE ON A CLEAN PROTECTED SURFACE. 2. REPLACE INNER SEAT ADJUSTER(S) WITH NEW ADJUSTER(S). PART NO. SEAT ADJ. -------- --------- 20329374 PASSENGER OUTER (COUPE) 20329375 PASSENGER OUTER (SEDAN) 20162884 PASSENGER INNER (COUPE) 20162885 PASSENGER INNER (SEDAN) NOTE IF 20162885 INTERFERS WITH CONSOLE USE P/N 20329275 20330804 DRIVERS' INNER (COUPE) 20330805 DRIVERS' INNER (SEDAN) 3. INSTALL RELEASE WIRE (20162898) BETWEEN LOCK BARS. 4. IF THE ADJUSTER TO FLOOR ATTACHING STUD IS LOOSE IN THE FLOOR, WELD THE STUD (MIG OR GAS WITH STEEL ROD ONLY) INTO PLACE USING STANDARD BODY SHOP REPAIR PROCEDURE FOR STRUCTUAL COMPONENTS. 5. INSTALL SEAT TO FLOOR AND TORQUE SEAT ADJUSTER-TO-FLOOR PAN ATTACHING NUTS 20 TO 28 N.M (15 TO 21 FT-LB).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.