OIL LEAK AT OIL PAN GASKET LOCTITE USAGE. Buick Skyhawk 1983

For 1990-2009 cars

# OIL LEAK AT OIL PAN GASKET LOCTITE USAGE

#### Models Affected: 1982-83-84 Skyhawks Equipped with 1.8L (Vin Code 0) Engines

Some comments have been received concerning oil leaks at the oil pan gasket on 1.8L OHC engines as well as loose pan bolts.

When it is found that the oil leak at the oil pan is caused by loose pan bolts, remove the bolts and apply Loctite or equivalent to the thread area and reinstall the bolts. The torque specifications for the pan bolts is 5N.m (41 b.ft.).

The pan installation procedure is found on page 6A2-13 of the 1984 Service Manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.