REAR MAIN OIL SEAL REPLACEMENT INFORMATION. Buick Skyhawk 1982

For 1990-2009 cars

# REAR MAIN OIL SEAL REPLACEMENT INFORMATION

THE FOLLOWING PRECAUTION SHOULD BE TAKEN WHEN APPLYING SEALER TO THE LOWER REAR MAIN CAP AREA ON SUBJECT ENGINES: APPLY A 2MM BEAD OF ANEROBIC SEALANT(PART NO. 1052357)OR EQUIVALENT TO THE BEARING CAP AS SHOWN IN FIGURE 22. KEEP SEALANT OFF THE SEAL, BEARING, AND OUT OF DRAIN SLOT.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.