EXCESSIVE EFFORT TO SHIFT CABLE SYSTEM ROUTING INFO. Buick Skyhawk 1982

For 1990-2009 cars

# EXCESSIVE EFFORT TO SHIFT CABLE SYSTEM ROUTING INFO

EXCESSIVE EFFORT TO OPERATE THE SHIFT LEVER AND/OR DIFFICULTY IN REMOVING THE IGNITION KEY FROM THE STEERING COLUMN ON 1982 FIRENZA MODELS MAY BE CAUSED BY THE PARK LOCK CABLE SYSTEM. WHEN ATTEMPTING TO CORRECT EITHER OF THESE CONDITIONS, CHECK THE PARK LOCK CABLE FOR PROPER ROUTING, KINKS, AND PROPER ADJUSTMENT. REFER TO PAGE 7A-3 OF THE 1982 FIRENZA SERVICE MANUAL FOR ADJUSTMENT PROCEDURE.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.