For 1990-2009 cars

## DTC P0503 Vehicle Speed Sensor (VSS) Circuit Intermittent 2.4L VIN T

Handling ESD Sensitive Parts Notice
OBD II Symbol Description Notice
Automatic Transmission Controls Schematics 2.4L VIN T
Automatic Transmission Components 2.4L VIN T

### Circuit Description

The Vehicle Speed Sensor (VSS) is a Permanent Magnet (PM) generator attached to the transmission case extension. The final drive assembly has a toothed wheel (VSS rotor). As the final drive assembly rotates, an AC voltage is induced and transmitted to the Powertrain Control Module (PCM).

The PCM converts the induced AC voltage into a digital signal. The PCM uses the vehicle speed in order to determine the shift timing, the TCC apply and release, and the gear ratio calculations. The VSS voltage varies from 0.5 volts AC at 100 RPM to more than 100 volts AC at 6000 RPM. The VSS resistance is 981-1864 ohms.

If the PCM detects a low vehicle speed with a high engine speed while in a drive range, then DTC P0503 sets. DTC P0503 is a type A DTC.

### Conditions for Setting the DTC

• | The engine speed is more than 500 RPM for 5 seconds.

• | The engine is not in fuel shut off.

• | More than 6 seconds has elapsed since the last gear change.

• | The output speed does not rise more than 1000 RPM within 2 seconds.

• | The transmission is not in Park or Neutral.

• | The output speed drops more than 1500 RPM within 2 seconds.

### Action Taken When the DTC Sets

• | The transmission defaults to 3rd gear.

• | The PCM inhibits TCC operation.

• | The PCM illuminates the Malfunction Indicator Lamp (MIL).

### Conditions for Clearing the MIL/DTC

• | The PCM turns OFF the MIL after three consecutive ignition cycles without a failure reported.

• | A scan tool can clear the DTC from the PCM history. The PCM clears the DTC from the PCM history if the vehicle completes 40 warm-up cycles without a failure reported.

• | The PCM cancels the DTC default actions when the fault no longer exists and the ignition is OFF long enough in order to power down the PCM.

### Diagnostic Aids

• | Inspect the wiring for poor electrical connections at the PCM. Inspect the wiring at the transmission 7-way connector. Look for the following conditions:

- | A bent terminal

- | A backed out terminal

- | A damaged terminal

- | Poor terminal tension

- | A chafed wire

- | A broken wire inside the insulation

• | When diagnosing for an intermittent short or open condition, massage the wiring harness while watching the test equipment for a change.

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. This step verifies that the PCM is receiving a signal from the vehicle speed sensor.

2. This step verifies that no open exists in the circuitry from the vehicle speed sensor to the PCM connector.

3. This step performs a resistance test on the VSS circuits from the PCM connector.

#### DTC P0503 ('96 Ncar, 2.4L, 4T60-E)

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Powertrain On-Board Diagnostic (OBD) System Check performed? | -- | Go to Step 2 | Go to Powertrain On Board Diagnostic (OBD) System Check
2 |

1. Install the scan tool.
2. With the engine OFF, turn the ignition switch to the RUN position.

Important: Before clearing the DTCs, use the scan tool in order to record the Freeze Frame and Failure Records for reference. The Clear Info function erases the stored Freeze Frame and Failure Records from the PCM.

3. Record the DTC Freeze Frame and Failure Records.

Notice: Support the lower control arms in the normal horizontal position in order to avoid damage to the drive axles. Do not operate the vehicle in gear with the wheels hanging down at full travel.

4. Raise and support the drive wheels.
5. Start and idle the engine.
6. Place the transmission in drive range.
7. Select Output Speed on the scan tool.

With the drive wheels rotating, does the transmission output speed increase as the wheel speed increases?

--

Go to Diagnostic Aids

Go to Step 3

3 |

1. Turn the ignition switch OFF.
2. Disconnect PCM connector C1.
3. Connect the J 39200 DMM from terminal C1-64 to terminal C2-61 of the PCM connector.
4. Select AC volts on the DMM.
5. Rotate the drive wheels.

Is the voltage greater than the specified value?

0.5V

Go to Step 4

Go to Step 6

4 | Use the scan tool in order to find the most current calibration ID. Refer to Service Bulletins. Does the ID number match? | -- | Go to Step 13 | Go to Step 5
5 | Update the PCM with the latest calibration. Refer to Powertrain Control Module/EEPROM Replacement/Programming , Section 6. Is the calibration update complete? | -- | Go to Step 14 | --
6 |

1. Remove the VSS. Refer to Vehicle Speed Sensor, in On-Vehicle Service.
2. Connect the J 39200 DMM from terminal A to terminal B of the VSS.
3. Select ohms on the DMM.

Is the measured resistance within the specified range?

981-1864ohms

Go to Step 7

Go to Step 12

7 |

1. Install the VSS. Refer to Vehicle Speed Sensor, in On-Vehicle Service.
2. Connect the J 39200 DMM from terminal C1-64 to terminal C2-61 of the PCM connector.
3. Select ohms on the DMM.

Is the measured resistance greater than the specified value?

1864ohms

Go to Step 8

Go to Step 9

8 |

1. Inspect circuit 400 and circuit 401 for an open.
2. Repair the circuits if necessary.

Refer to Troubleshooting Procedures, Section 8.

Did you find and correct a problem?

--

Go to Step 14

--

9 | Does the J 39200 DMM display a value less than the resistance specified? | 981ohms | Go to Step 10 | Go to Step 11
10 |

1. Inspect circuits 400 and 401 for a short together.
2. Repair the circuits if necessary.

Refer to Troubleshooting Procedures, Section 8.

Did you find and correct a problem?

--

Go to Step 14

--

11 |

1. Inspect circuits 400 and 401 for a short to ground.
2. Repair the circuits if necessary.

Refer to Troubleshooting Procedures, Section 8.

Did you find and correct a problem?

--

Go to Step 14

Go to Step 13

12 | Replace the VSS. Refer to Vehicle Speed Sensor Replacement, in On-Vehicle Service. Is the replacement complete? | -- | Go to Step 14 | --
13 | Replace the PCM. Refer to Powertrain Control Module/EEPROM Replacement/Programming , Section 6. Is the replacement complete? | -- | Go to Step 14 | --
14 | In order to verify your repair, perform the following procedure:

1. Select DTC.
2. Select Clear Info.
3. Operate the vehicle under the following conditions:

• | The engine speed more than 500 RPM for 5 seconds

• | The engine is not in fuel shut off.

• | More than 6 seconds has elapsed since the last gear change.

• | The output speed does not drop more than 500 RPM within 5 seconds.

• | The output speed is more than 1000 RPM for 2 seconds.

4. Select Specific DTC. Enter DTC P0503.

Has the test run and passed?

--

System OK

Begin the diagnosis again. Go to Step 1

## DTC P0503 Vehicle Speed Sensor (VSS) Circuit Intermittent 3.1L VIN M

Handling ESD Sensitive Parts Notice
OBD II Symbol Description Notice
Automatic Transmission Controls Schematics 3.1L VIN M
Automatic Transmission Components 3.1L VIN M

### Circuit Description

The Vehicle Speed Sensor (VSS) is a Permanent Magnet (PM) generator attached to the transmission case extension. The final drive assembly has a toothed wheel (VSS rotor). As the final drive assembly rotates, an AC voltage is induced and transmitted to the Powertrain Control Module (PCM).

The PCM converts the induced AC voltage into a digital signal. The PCM uses the vehicle speed in order to determine the shift timing, the TCC apply and release, and the gear ratio calculations. The VSS voltage varies from 0.5 volts AC at 100 RPM to more than 100 volts AC at 6000 RPM. The VSS resistance is between 1300 and 1950 ohms.

If the PCM detects a low vehicle speed with a high engine speed while in a drive range, then DTC P0503 sets. DTC P0503 is a type A DTC.

### Conditions for Setting the DTC

• | The engine speed is more than 500 RPM for 5 seconds.

• | The engine is not in fuel shut off.

• | More than 6 seconds has elapsed since the last gear change.

• | The output speed does not rise more than 1000 RPM within 2 seconds.

• | The transmission is not in Park or Neutral.

• | The output speed drops more than 1500 RPM within 2 seconds.

### Action Taken When the DTC Sets

• | The transmission defaults to 3rd gear.

• | The PCM inhibits TCC operation.

• | The PCM illuminates the Malfunction Indicator Lamp (MIL).

### Conditions for Clearing the MIL/DTC

• | The PCM turns OFF the MIL after three consecutive ignition cycles without a failure reported.

• | A scan tool can clear the DTC from the PCM history. The PCM clears the DTC from the PCM history if the vehicle completes 40 warm-up cycles without a failure reported.

• | The PCM cancels the DTC default actions when the fault no longer exists and the ignition is OFF long enough in order to power down the PCM.

### Diagnostic Aids

• | Inspect the wiring for poor electrical connections at the PCM. Inspect the wiring at the TCC brake switch. Look for the following conditions:

- | A bent terminal

- | A backed out terminal

- | A damaged terminal

- | Poor terminal tension

- | A chafed wire

- | A broken wire inside the insulation

• | When diagnosing for an intermittent short or open condition, massage the wiring harness while watching the test equipment for a change.

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. This step verifies that the PCM is receiving a signal from the vehicle speed sensor.

2. This step verifies that no opens exist in the circuitry from the vehicle speed sensor to the PCM connector.

3. This step performs a resistance test on the VSS circuits from the PCM connector.

#### DTC P0503 Vehicle Speed Sensor Circuit (VSS) Low Input

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Powertrain On-Board Diagnostic (OBD) System Check performed? | -- | Go to Step 2 | Go to Powertrain On Board Diagnostic (OBD) System Check
2 |

1. Install the scan tool.
2. With the engine OFF, turn the ignition switch to the RUN position.

Important: Before clearing the DTCs, use the scan tool in order to record the Freeze Frame and Failure Records for reference. The Clear Info function erases the stored Freeze Frame and Failure Records from the PCM.

3. Record the DTC Freeze Frame and Failure Records.

Notice: Support the lower control arms in the normal horizontal position in order to avoid damage to the drive axles. Do not operate the vehicle in gear with the wheels hanging down at full travel.

4. Raise and support the drive wheels.
5. Start and idle the engine.
6. Place the transmission in drive range.
7. Select Output Speed on the scan tool.

With drive wheels rotating, does transmission output speed increase when wheel speed increases?

--

Go to Step 3

Go to Step 5

3 | Use the scan tool to find the most current calibration ID. Refer to Service Bulletins. Does the ID number match? | -- | Go to Step 5 | Go to Step 4
4 | Update the PCM with the latest calibration. Refer to Powertrain Control Module Replacement/Programming , Section 6. Is the calibration update complete? | -- | Go to Step 15 | --
5 |

1. Turn the ignition OFF.
2. Disconnect PCM connector C1.
3. Connect J 39200 DVOM from terminal 6 to terminal 47 of the PCM connector.
4. Select AC volts on the voltmeter.
5. Rotate the drive wheels and observe the display.

Is the measured voltage greater than the specified value?

0.5 v

Go to Step 9

Go to Step 6

6 |

1. Remove the VSS.
2. Connect J 39200 DVOM from terminal A to terminal B of the VSS.

Is the measured resistance within the specified range?

981ohms to 1864ohms

Go to Step 7

Go to Step 12

7 |

1. Install the VSS.
2. Connect J 39200 DVOM from terminal 6 to terminal 47 of the PCM connector.

Does the J 39200 DVOM display a value greater than the specified value?

1864ohms

Go to Step 8

Go to Step 9

8 |

1. Inspect circuit 400 and circuit 401 for an open.
2. Repair the circuits if necessary.

Refer to Troubleshooting Procedures, Section 8.

Did you find and correct a problem?

--

Go to Step 15

--

9 | Does the J 39200 DVOM display a value less than the resistance specified? | 981ohms | Go to Step 10 | Go to Step 11
10 |

1. Inspect circuits 400 and 401 for a short together.
2. Repair the circuits if necessary.

Refer to Troubleshooting Procedures, Section 8.

Did you find and correct a problem?

--

Go to Step 15

--

11 |

1. Inspect circuits 400 and 401 for a short to ground.
2. Repair the circuits if necessary.

Refer to Troubleshooting Procedures, Section 8.

Did you find and correct a problem?

--

Go to Step 15

Go to Step 13

12 | Replace the vehicle speed sensor. Refer to VSS Replacement, in On-Vehicle Service. Is the replacement complete? | -- | Go to Step 15 | --
13 |

1. Disconnect the C1 (Blue) connector form the Powertrain Control Module (PCM).
2. Inspect the PCM connector terminals for the following conditions:

• | Dammaged connector pins

• | Backed-out conncector pins

• | Weak terminal tension

Did you find and correct a problem?

--

Go to Step 15

Go to Step 14

14 | Replace the PCM. Refer to Powertrain Control Module Replacement/Programming , Section 6 Is the replacement complete? | -- | Go to Step 15 | --
15 | In order to verify your repair, perform the following procedure:

1. Select DTC.
2. Select Clear Info.
3. Operate the vehicle under the following conditions:

• | The engine speed more than 500 RPM for 5 seconds

• | The engine is not in fuel shut off.

• | More than 6 seconds has elapsed since the last gear change.

• | No output speed drop more than 500 RPM within 5 seconds.

• | Output speed is more than 1000 RPM for 2 seconds.

4. Select Specific DTC. Enter DTC P0503.

Has the test run and passed?

--

System OK

Begin the diagnosis again. Go to Step 1