For 1990-2009 cars

#### Tools Required

J 41352 Modular Column Holding Fixture

Caution: The tilt spring and the spring guide are under pressure. The tilt spring and the spring guide may become a projectile. Secure the spring with locking pliers during removal. Secure the spring with locking pliers during installation. Bodily injury may result during removal and installation of the tilt spring and the spring guide. Always use caution during removal and installation of the tilt spring and the spring guide.

1. Install the spring guide (1) into the tilt spring (2).
2. Insert the tilt spring into the steering column support assembly.

Important: The tabs on the spring retainer must fit inside of the steering column support assembly.

3. Secure the tilt spring (2) with the spring retainer (3) by applying pressure to the spring retainer and turning counterclockwise.
4. Release the pressure on the spring retainer (3) once the tabs are locked in place.
5. Remove the steering column from J 41352 .