For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Wiper/Washer System Check? | -- | Go to Step 2 | Go to Wiper/Washer System Check or Wiper/Washer System Check
2 |

1. Turn the ignition switch to RUN.
2. Turn the wiper switch to LOW.
3. Disconnect the wiper motor connector C1.
4. Connect a test lamp from connector C1, terminal F, to ground.
5. Momentarily activate and release the washer switch while observing the test lamp.

Does the test lamp light?

--

Go to Step 3

Go to Step 6

3 | Test for a short to B+ in CKT 94. Does a short to B+ exist? | -- | Go to Step 4 | Go to Step 5
4 | Repair the short to B+ in CKT 94. Did you complete the repair? | -- | Go to Wiper/Washer System Check or Wiper/Washer System Check | --
5 | Replace the wiper/washer switch. Refer to Windshield Wiper and Washer Switch Replacement - On Vehicle . Did you complete the repair? | -- | Go to Wiper/Washer System Check or Wiper/Washer System Check | --
6 | Replace the wiper motor cover. Refer to Wiper Motor Cover Replacement . Did you complete the repair? | -- | Go to Wiper/Washer System Check or Wiper/Washer System Check | --