For 1990-2009 cars

## Door Inside Handle Bezel Replacement Pontiac

### Removal Procedure

1. Remove the locking rod knob.
2. In order to remove the bezel (1) from the door inside handle, gently pry at the bottom corner and work around.
3. Rotate the bezel and pull forward in order to slide over the door handle.

### Installation Procedure

1. Install the bezel to the door inside handle by first inserting the door handle in the door handle opening.
2. Align the studs to the retainers and apply pressure on the bezel (1) in order to secure.
3. Install the locking rod knob.

## Door Inside Handle Bezel Replacement Oldsmobile and Buick

### Removal Procedure

1. Remove the locking rod knob.
2. In order to remove the bezel (1) from the door inside handle, gently pry at the bottom corner and work around.
3. Rotate the bezel and pull forward in order to slide over the door handle.

### Installation Procedure

1. Install the bezel to the door inside handle by first inserting the door handle in the door handle opening.
2. Align the studs to the retainers and apply pressure on the bezel (1) in order to secure.
3. Install the locking rod knob.