For 1990-2009 cars

CAUTION: The SIR driver deployment loop (circuits 347 and 348) passes through connector C200. You must take special precautions before servicing C200. Disable the SIR system before you disconnect, probe, or service connector C200. Refer to Disabling the SIR System in Restraints SCT 9. Failure to follow the correct procedure could cause air bag deployment, personal injury or unnecessary SIR system repairs.