For 1990-2009 cars

# INFO. ON ELIMINATION OF THE INERTIA LOCK FEATURE

#### SUBJECT: INFORMATION ON ELIMINATION OF THE INERTIA LOCK FEATURE FOR THE FRONT SEAT RECLINER

#### MODELS: 1996 BUICK SKYLARK COUPE 1996 CHEVROLET CAVALIER COUPE 1996 OLDSMOBILE ACHIEVA COUPE 1996 PONTIAC GRAND AM COUPE, SUNFIRE COUPE

THE INERTIA LOCK FEATURE OF THE FRONT SEAT RECLINER HAS BEEN ELIMINATED FROM THE FOLLOWING VEHICLES BUILT AFTER THE VIN BREAKPOINTS LISTED:

J-CAR: CHEVROLET - T7145765 (LORDSTOWN) ===== TM106531 (LANSING) TB101034 (GENASYS) TS847713 (RAMOS)

PONTIAC - T7517569 (LORDSTOWN) TB200860 (GENASYS) TS847716 (RAMOS)

N-CAR: BUICK TC403647 ===== OLDSMOBILE TM303293 PONTIAC TC710245 AND TM502734

J-CAR: =====

FOR VEHICLES BUILT BEFORE THE ABOVE VIN BREAKPOINTS WHICH HAVE FRONT SEAT RECLINERS WITH THE INERTIA LOCK FEATURE, USE P/N 16779872 FOR THE NON E-Z ENTRY PASSENGER SEAT RECLINER, P/N 16779874 FOR THE E-Z ENTRY PASSENGER SEAT RECLINER, AND P/N 16779875 FOR THE DRIVER SEAT RECLINER.

FOR VEHICLES BUILT AFTER THE ABOVE VIN BREAKPOINTS WHICH HAVE FRONT SEAT RECLINERS WITHOUT THE INERTIA LOCK FEATURE, PLEASE NOTE THE FOLLOWING:

- USE P/N 16800034 FOR THE NON E-Z ENTRY PASSENGER SEAT RECLINER, P/N 16802910 FOR THE E-Z ENTRY PASENGER SEAT RECLINER AND P/N 16802911 FOR THE DRIVER SEAT RECLINER.

- THE RELEASE LATCH LOCATED AT THE LOWER OUTER CORNER OF THE BACK SIDE OF THE SEATBACK MUST BE LIFTED TO FOLD THE SEATBACK TO THE FORWARD POSITION.

- THE SERVICE PROCEDURE TO REMOVE AND REPLACE THE RECLINER HAS NOT CHANGED.

- DISREGARD ANY INERTIA LOCK INFORMATION IN SECTION 10-10 OF THE SERVICE MANUAL.

N-CAR: =====

FOR VEHICLES BUILT BEFORE THE ABOVE VIN BREAKPOINTS WHICH HAVE FRONT SEAT RECLINERS WITH THE INERTIA LOCK FEATURE, USE P/N 16780386 FOR THE PASSENGER SEAT RECLINER AND P/N 16780387 FOR THE DRIVER SEAT RECLINER.

FOR VEHICLES BUILT AFTER THE ABOVE VIN BREAKPOINTS WHICH HAVE FRONT SEAT RECLINERS WITHOUT THE INERTIA LOCK FEATURE, PLEASE NOTE THE FOLLOWING:

- USE P/N 16800068 FOR THE PASSENGER SEAT RECLINER AND P/N 16802911 FOR THE DRIVER SEAT RECLINER.

- THE RELEASE LATCH LOCATED AT THE LOWER OUTER CORNER OF THE BACK SIDE OF THE SEATBACK MUST BE LIFTED TO FOLD THE SEATBACK TO THE POSITION.

- THE SERVICE PROCEDURE TO REMOVE AND REPLACE THE RECLINER HAS NOT CHANGED.

- DISREGARD ANY INERTIA LOCK INFORMATION IN SECTION 10-10 OF THE SERVICE MANUAL.

SOME OWNERS MAY COMMENT THAT THEIR FRONT SEAT DOES NOT OPERATE AS STATED IN THE OWNER'S MANUAL. ADVISE THE OWNER THAT THE FRONT SEAT RECLINER INFORMATION IN THE OWNER'S MANUAL, WHICH RECOMMENDS THE OWNER TO SIMPLY PUSH THE FRONT SEATBACK TO FOLD THE SEATBACK FORWARD, DOES NOT APPLY TO THEIR VEHICLE. ADVISE THE OWNER TO LIFT THE RELEASE LATCH TO POSITION THE FRONT SEATBACK IN THE FORWARD POSITION.

#### PARTS INFORMATION:

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1996 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.