For 1990-2009 cars

Application | Fluid/Lubricant
--- | ---
Automatic Transaxle | DEXRON®-III Automatic Transmission Fluid (or equivalent)
Engine Coolant | A 50/50 mixture of clean water (preferably distilled) and use only GM Goodwrench® DEX-COOL® or Havoline® DEX-COOL® (orange-colored, silicate-free) coolant, conforming to GM Specification 6277M
Chassis Lubrication | Chassis Lubricant aerosol (GM P/N 1052497 or equivalent) or lubricant meeting the requirements of NLGI # 2, Category LB or GC-LB
Engine Oil | Engine Oil with the American Petroleum Institute Certified For Gasoline Engines STARBURST symbol of the proper viscosity. SAE 5W-30 is best for the vehicle. However, SAE 10W-30 can be used if the temperature is 0°F (-18°C) or above.
Manual Transaxle | Synchromesh Transmission Fluid (GM P/N 12345349)
Hood Latch, Pivots, and Spring Anchor | Lubriplate Lubricant aerosol (GM P/N 1052497 or equivalent) or a lubricant meeting the requirements of NLGI # 2, Category LB or GC-LB
Hood Release Pawl | Lubriplate Lubricant aerosol (GM P/N 1052497 or equivalent) or a lubricant meeting the requirements of NLGI # 2, Category LB or GC-LB
Hydraulic Brake System | Delco Supreme 11® Brake Fluid (GM P/N 1052535) or equivalent DOT-3 brake fluid
Hydraulic Clutch System | Hydraulic Clutch Fluid (GM P/N 12345347 or equivalent)
Key Lock Cylinders | Multi-Purpose Lubricant, Superlube® (GM P/N 12345120 or equivalent)
Manual Transaxle | Synchromesh Transmission Fluid (P/N 12345349)
Parking Brake Cable Guides, Underbody Contact Points and Linkage | Chassis lubricant (GM P/N 1052497) or lubricant meeting the requirements of NLGI # 2, Category LB or GC-LB
Power Steering System | GM Hydraulic Power Steering Fluid (GM P/N 1052884 or equivalent)
Weatherstrip Conditioning | Dielectric Silicone Grease (GM P/N 12345579 or equivalent)
Windshield Washer Solvent | GM Optikleen® Washer Solvent (GM P/N 1051515 or equivalent)
Automatic Transaxle Shift Linkage | Engine Oil