For 1990-2009 cars

## Window Channel Replacement Front

### Removal Procedure

1. Remove the door trim panel. Refer to Door Trim Panel Replacement .
2. Remove enough door water deflector in order to access the upper window run channel. Refer to Door Water Deflector Replacement
3. Raise the window to the full up position.
4. Remove the door speaker. Refer to Radio Front Side Door Speaker Replacement in Entertainment.
5. Remove the upper window run channel bolt (1).
6. Lower the window to the full down position.
7. Remove the upper window run channel (2).

### Installation Procedure

1. Install the upper window run channel (2).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolt (1) to the upper window run channel.

Tighten
Tighten the bolt to 9 N·m (80 lb in).

3. Install the door speaker. Refer to Radio Front Side Door Speaker Replacement in Entertainment.
4. Install the door water deflector. Refer to Door Water Deflector Replacement .
5. Install the door trim panel. Refer to Door Trim Panel Replacement .

## Window Channel Replacement Rear

### Removal Procedure

1. Remove the door trim panel. Refer to Door Trim Panel Replacement .
2. Remove enough door water deflector in order to access the upper window run channel. Refer to Door Water Deflector Replacement .
3. Raise the window to the full up position.
4. Remove the door speaker. Refer to Radio Rear Speaker Replacement in Entertainment.
5. Remove the upper window run channel bolt (2).
6. Remove the upper window run channel screw (1).
7. Lower the window to the full down position.
8. Remove the upper window run channel.

### Installation Procedure

1. Install the upper window run channel.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolt (2) to the upper window run channel.

Tighten
Tighten the bolt to 9 N·m (80 lb in).

3. Install the upper window run channel screw (1).
4. Install the door speaker. Refer to Radio Rear Speaker Replacement in Entertainment.
5. Install the door water deflector. Refer to Door Water Deflector Replacement .
6. Install the door trim panel. Refer to Door Trim Panel Replacement .