For 1990-2009 cars

# 125-125C ROUGH NEUTRAL TO DRIVE, NEW CLUTCH WAVE PLATE

#### MODELS AFFECTED: ALL 1982 THRU 1984 THM 125/125-C TRANSAXLES

#### NOTE: This Bulletin supercedes Bulletin 84-7125-2. Please discard previous bulletin and replace it with this one. Serial number break points were incorrect in the original bulletin.

Some 1982 thru 1984 THM 125/125-C transaxles may exhibit a rough neutral to drive shift condition.

Beginning in Decenber, 1983, a new forward clutch wave plate, part number 8652126 went into production on THM 125C model transaxles. The chart below provides model and serial number break points for installation of the new wave plate on 1984 models. All 1982 and 1983 models and all 1984 units assembled prior to these break points have the past model wave plate.

Therefore, when servicing any 1982 thru 1984 model THM 125/125C transaxles for this harsh neutral to drive condition the new wave plate part number 8652126 should be installed. Refer to the appropriate service manual for removal and replacement instructions.

#### MODEL SERIAL NO. MODEL SERIAL NO. ----- ---------- ----- ---------- CA 2724 PD 2508 CB 221301 PE 64573 CE 77876 PF 31776 CF 7881 PG 63043 CR 4840 PJ 8148 PW 82620

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.