For 1990-2009 cars

Application | N·m | Lb Ft | Lb In.
--- | --- | --- | ---
Battery Retainer Bolt | 18 | 13 | --
Commutator End Frame/Field Frame Assembly Through Bolts | 8.5 | -- | 75
Front Generator Bracket to Block Attaching Bolt (3.1L) | 50 | 37 | --
Generator Rear Mounting Bolt (3.1L) | 25 | 18 | --
Ignition Wire Harness Bracket Nut (3.1L) | 13 | 10 | --
Ignition Wire Harness Retaining Bolt (3.1L) | 25 | 18 | --
Negative Battery to Transaxle Stud Nut | 30 | 22 | --
Battery Cable to Battery Bolt | 16 | 12 | --
Positive Battery Cable to Generator Nut | 7.5 | -- | 65
Positive Battery Cable to Starter Solenoid Nut | 12 | -- | 106
Generator to bracket bolt (2.4L) | 50 | 37 | --
Solenoid Attaching Screws | 11 | -- | 95
Spark Plugs (2.4L) | 18 | 13 | --
Spark Plugs (3.1L) | 20 | 15 | --
Starter Field Lead to Solenoid Attaching Screw | 9.5 | -- | 84
Starter Lead Wire to Starter Solenoid S Terminal Nut | 2.5 | -- | 22
Starter Motor to Engine Bolt (2.4L) | 90 | 66 | --
Starter Motor to Engine Bolt (3.1L) | 43 | 32 | --