For 1990-2009 cars

## Upper Extension Trim Panel Replacement Oldsmobile and Buick

### Removal Procedure

Remove the upper trim panel (1) from the front door by gently prying at the side. Disengage the tabs and pull the panel rearward.

### Installation Procedure

Install the upper trim panel (1) to the front door by inserting the tabs to the retainers and applying pressure.

## Upper Extension Trim Panel Replacement Pontiac

### Removal Procedure

1. Remove the upper trim panel (1) from the front door by gently prying at the side. Disengage the tabs and pull the panel rearward.
2. Remove the speaker wiring lead (3) from the speaker connector (2).

### Installation Procedure

1. Install the speaker wiring lead (3) to the speaker connector (2).
2. Install the upper trim panel (1) to the front door by inserting the tabs to the retainers and applying pressure.