For 1990-2009 cars

### Removal Procedure

#### Tools Required

• | J 6125-1B Slide Hammer

• | J 23129 Axle Boot Remover

1. Raise the vehicle. Support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Drain the oil.
3. Remove the oil pan attaching bolts, oil pan, and the gasket. Refer to Oil Pan Replacement .
4. Remove the oil filter. Use a long screwdriver in order to pry the filter neck out of the seal.
5. Remove the seal. Use the J 6125-1B and the J 23129 .
6. Check the oil filter seal for damage or wear.

### Installation Procedure

1. Install the new oil filter and the seal.
2. Install the oil pan gasket, oil pan and the attaching bolts. Refer to Oil Pan Replacement .
3. Lower the vehicle.
4. Fill the transmission to the proper level with DEXRON® III oil.
5. Inspect the oil pan gasket for leaks.