For 1990-2009 cars

# 2ND GEAR STARTS 125/125C TRANS MISSION CONTROL VALVE ASSEMBLY

#### MODELS AFFECTED: 1982 & 1983 CE MODEL ONLY AND ALL 1984 MODEL THM 125/125-C TRANSAXLES

Some 1982, and 1983, CE model only, and early 1984 model THM 125/125-C transaxles may exhibit a second gear start, which is best described as the transaxle starting in second gear range instead of first gear range.

Starting with the serial numbers listed below a new control valve body assembly went into production to correct this second gear start conditiion.

When servicing any 1982 or 1983 CE model only, or early 1984 model THM 125/125-C transaxle for this second gear start condition, replace the control valve body assenbly with the control valve body assenbly listed in the dealership parts manual.

#### MODEL SERIAL NO. MODEL SERIAL NO. ----- ---------- ----- ----------

CA 1674 PD 2104 CB 91946 PE 42048 CE 47452 PF 13478 CF 4607 PG 36699 CT 3519 PJ 4822 PW 47580

#### MODEL JULIAN DATE ----- ----------- BF 005 BL 005 OP 005

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.