For 1990-2009 cars

### Removal Procedure

Typical EGR Valve shown.

1. Disconnect the electrical connector at the EGR valve (2).
2. Remove the 2 fasteners (1) from the EGR valve.
3. Remove the EGR valve (2).

### Installation Procedure

Typical EGR Valve shown.

1. Install the EGR valve (2).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the 2 EGR valve fasteners (1).

Tighten
Tighten the nuts to 30 N·m (22 lb ft).

3. Connect the electrical connector.