For 1990-2009 cars

### Removal Procedure

1. Remove the wheel housing. Refer to Wheelhouse Panel Replacement .
2. Remove the screw (2) from the fender sound insulator.
3. Remove the retainer (3) from the fender sound insulator.
4. Remove the fender sound insulator (1).

### Installation Procedure

1. Install the fender sound insulator (1).
2. Install the retainers (3) to the fender sound insulator.
3. Install the screws (2) to the fender sound insulator.
4. Install the wheel housing. Refer to Wheelhouse Panel Replacement .