For 1990-2009 cars

# SMU-Revised DTC P0101

Subject: | Revised DTC P0101

Models: | 1996-98 Skylark

| 1996-99 Buick Century, Regal

| 1996 Chevrolet Beretta, Corsica

| 1996-99 Lumina, Monte Carlo, Venture

| 1997-99 Chevrolet Malibu

| 1996 Oldsmobile Cutlass Ciera

| 1996-97 Oldsmobile Cutlass Supreme

| 1996-98 Oldsmobile Achieva

| 1996-99 Oldsmobile Silhouette

| 1997-98 Oldsmobile Cutlass

| 1999 Oldsmobile Alero

| 1996-99 Pontiac Grand Am, Grand Prix, Trans Sport

| 1999 Pontiac Montana

| with 3.1L or 3.4L Engine (VINs J, M, X, E - RPOs LG8, L82, LQ1, LA1)

This bulletin is being issued to revise DTC P0101 in the Engine Controls sub-section of the Service Manual. Please replace the current information in the Service Manual with the following information.

The following information has been updated within SI2000. If you are using a paper version of this Service Manual, please make a reference to this bulletin on the affected page.

The text in Steps 7 or 9 (depending on the model) in DTC P0101 has been revised to read "Does the scan tool parameter go from 0 to 100%?".