For 1990-2009 cars

### Surge Tank Cap Pressure Test

#### Tools Required

• | J 24460-01 Cooling System and Cap Pressure Tester

• | J 24460-92 Cooling System Tester Adapter

1. Inspect the surge tank cap for loss of pressure using the J 24460-92 and the J 24460-01 . If the surge tank cap does not hold 103 kPa (15 psi), replace the cap.
2. Use the correct pressure cap. Use only a 103 kPa (15 psi) pressure cap.