For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Compressor and Condenser Hose Bolt | 33 N·m | 24 lb ft
A/C Pressure Transducer | 5 N·m | 44 lb in
A/C Receiver Dehydrator Tube Retaining Clamp Bolt | 10 N·m | 89 lb in
Compressor Bolts - 2.4L and 3.1L | 50 N·m | 37 lb ft
Compressor Crankcase Bolt | 20 N·m | 15 lb ft
Condenser Inlet Fitting | 28 N·m | 21 lb ft
Condenser Outlet Fitting | 28 N·m | 21 lb ft
Condenser to Radiator Screws | 6 N·m | 53 lb in
Evaporator Clamp Screw | 1.4 N·m | 12 lb in
Evaporator Inlet Fitting | 19 N·m | 14 lb ft
Evaporator Outlet Fitting | 48 N·m | 35 lb ft
Heater and A/C Module Nuts | 3 N·m | 27 lb in
Heater Core Cover Screws | 1.4 N·m | 12 lb in
Heater Core Screws | 1.4 N·m | 12 lb in
Heater Core Shroud Screws | 1.4 N·m | 12 lb in
Mode Valve Shaft Retainer Screw | 1.4 N·m | 12 lb in
Receiver Dehydrator Bracket Bolt | 10 N·m | 89 lb in
Receiver Dehydrator Inlet Fitting | 28 N·m | 21 lb ft
Receiver Dehydrator Outlet Fitting | 28 N·m | 21 lb ft
TXV Fitting from Evaporator Inlet Line | 17 N·m | 13 lb ft
TXV Fitting from Evaporator Outlet | 8 N·m | 71 lb in
TXV Fitting to Evaporator | 24 N·m | 17 lb ft