For 1990-2009 cars

### Assembly Procedure

Important: Replace the bearing and housing assembly and the picot pins if the bearing and housing assembly has been staked 3 times.

1. Install the bearing and housing assembly.
2. Lubricate the pivot pins with lithium grease.
3. Install the 2 pivot pins.
4. Stake the pivot pins in 3 locations.
5. Install the tilt spring. Refer to Tilt Spring - Assemble - Off Vehicle .
6. Install the ignition lock housing assembly. Refer to Lock Housing Assembly - Assemble - Off Vehicle .
7. Install the Ignition switch assembly. Refer to Ignition Switch Assembly - Assemble - Off Vehicle .
8. Install the upper tilt head components assembly. Refer to Steering Column Tilt Head Housing - Assemble - Off Vehicle .