For 1990-2009 cars

1. Inspect the 1-2 support roller clutch components for the following conditions:

• | A scored or burned contact surface for the manual 2-1 band on the 1-2 support drum (687)

• | A damaged or worn forward drum bushing

• | A damaged or worn inner race of the 1-2 support roller clutch

• | A damaged or worn 1-2 clutch roller assembly (683)

• | A damaged thrust bearing (685)

2. Install the 1-2 clutch roller assembly (683) into the 1-2 support drum.

Important: Note the position of the cage assembly to the inner race.

3. Install the thrust bearing (685) onto the 1-2 support drum (687). Press down with hand pressure only.