For 1990-2009 cars

# SERVICE MANUAL UPDATE SEC. 6E3 WIRING DIAGRAM CORRECTIONS

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 6E3 WIRING DIAGRAM CORRECTIONS

VEHICLES AFFECTED: 1992 "N" MODELS WITH 3.3L ENGINE (VIN N - RPO LG7)

This bulletin updates the following pages in the 1992 "N" Carline 3.3L (VIN N) Service Manual:

- ECM Wiring Diagram (3 of 3) 6E3-A-6 - Facing Page Art for Diagnostic Circuit Check 6E3-A-l0 - Facing Page Art for Chart A-1 6E3-A-l6 - Facing Page Art for Chart A-2 6E3-A-18 - Facing Page Art for Code 16 Chart 6E3-A-40 - Facing Page Art for Code 34 Chart 6E3-A-58

Also, CIRCUIT 439/ERLS FUSE should be changed to CIRCUIT 639/IGNITION ECM FUSE on the following pages:

- Chart A-1, Chart 6E3-A-16,17 - Code 34, Chart 6E3-A-59 - ECM Symptom Chart (3 of 6) 6E3-B-21

Please make the appropriate changes to the 1992 'N' Carline 3.3L (VIN N) Service Manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.