For 1990-2009 cars

# SERVICE MANUAL UPDATE SEC. 3C FRONT SUSPENSION HUB SEAL TOOL

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 3C FRONT SUSPENSION (INNER HUB SEAL INSTALLER ART WORK LABELED WITH CORRECT TOOL NUMBER)

#### MODELS AFFECTED: 1991 SKYLARKS

#### SERVICE MANUAL UPDATE

Section 3C

The 1991 Skylark Service Manual improperly labels the Inner Hub Seal Installer. The correct tool number is J 34658.

The following art for this tool #J 34658 replaces the current art shown. Reference to the tool number must also be corrected on the following pages in the text.

#### TEXT ILLUSTRATION

3C-8, 3C-10 3C-16

Please correct your copy of the Service Manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.