For 1990-2009 cars

## Cylinder Head Removal Left Side

1. Remove the oil level indicator assembly retaining bolt.
2. Remove the oil level indicator assembly.
3. Remove the cylinder head bolts.
4. Remove the cylinder head assembly.
5. Remove the cylinder head gasket.

## Cylinder Head Removal Right Side

1. Remove the cylinder head bolts.
2. Remove the cylinder head assembly.
3. Remove the cylinder head gasket.