For 1990-2009 cars

# TRANSMISSION SIDE COVER BOLT & WASHER REPLACEMENT

#### MODELS AFFECTED: ALL THM TRANSMISSIONS OR TRANSAXLES

When servicing any THM transmission or transaxle and removal of the side cover and/or bottom pan is required, IT IS NOT ALWAYS NECESSARY TO REPLACE THE HEX HEAD SCREWS AND CONICAL WASHER ASSEMBLIES.

Only screws with the coating stripped away exposing exterior portion of the head or washer or those screws with the washer inverted should be replaced. (See illustration below ).

Insert this information in the appropriate section of your 1985 service manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.