For 1990-2009 cars

Condition | Causes
--- | ---
Increase in Effort While Turning Steering Wheel |

• | A hose is pinched.

• | A hose is restricted.

• | The flow control valve is sticking.

• | The steering pump reservoir has a low fluid level.

• | In cold weather, cold climate power steering fluid needs to be added.

• | The steering gear has an internal leak.

• | The power steering pump has an internal leak.